This folder contains AVR Firmware for FlashcatUSB.
Loading these firmwares will change the base functionality of FlashcatUSB.
For instructions on how to change firmware, please read the enclosed Documentation.
-----------------------------------------------

FCUSB.x.xx.SPI: Allows programming of high-density SPI flash devices.
FCUSB.x.xx.EJTAG: Allows programming of CFI devices over JTAG using DMA or PrAcc mode.
FCUSB.x.xx.NAND: Allows NAND programming over a SPI bus.

-----------------------------------------------
Please note, there are now two main branches of FlashcatUSB firmware depending on which PCB version you have.

Thank you for choosing Embedded Computers!
www.EmbeddedComputers.net